IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView]"
File name: "2. Faux plaf mur_int - vals plaf bi_muur.blend.ifc"
Time stamp: "2020-12-22T11:07:41+01:00"
Preprocessor: "IfcOpenShell 0.6.0b0"
Originating system: "BlenderBIM 0.0.200912"
Authorization: "Nobody"

Units
  LENGTHUNIT: CENTI METRE
  AREAUNIT: CENTI SQUARE_METRE
  VOLUMEUNIT: CENTI CUBIC_METRE

Spatial structure
IFCPROJECT "Default"
  IFCSITE "Default" | postal address OFFICE
    IFCBUILDING "Default" | postal address OFFICE
      IFCBUILDINGSTOREY "0" | elevation 1.91459258570865E-09
        contains 5 elements
          2 x IFCCOVERING | CEILING | names: "Faux plafond - verlaagd plafond" | material: "Plâtre plaque" | property sets: Pset_CoveringCommon, Cpset_Covering, Qto_CoveringBaseQuantities, Cpset_Ceiling
          2 x IFCCOVERING | CLADDING | names: "Enduit - bepleistering" | material: "Enduit cimenté blanc" | property sets: Pset_CoveringCommon, Cpset_Covering, Qto_CoveringBaseQuantities
          1 x IFCWALL | SOLIDWALL | names: "Maçonnerie portante - metselwerk" | material: "Bloc béton - 19 cm" | property sets: Pset_WallCommon, Cpset_Wall, Cpset_PrecastConcreteElement, Cpset_ConcreteElementGeneral, Qto_WallBaseQuantities
      IFCBUILDINGSTOREY "1"
        contains 7 elements
          1 x IFCCOVERING | MEMBRANE | names: "Pare-vapeur - vochtwerende folie" | material: "Membrane étanche" | property sets: Pset_CoveringCommon, Cpset_Covering, Qto_CoveringBaseQuantities
          3 x IFCSLAB | FLOOR | names: "Hourdis - prefab element", "Dalle de compression - druklaag" | material: "Hourdis"; "Chape de compression" | property sets: Pset_SlabCommon, Cpset_Slab, Cpset_ConcreteElementGeneral, Cpset_PrecastConcreteElement, Qto_SlabBaseQuantities, Pset_PrecastSlab
          2 x IFCCOVERING | FLOORING | names: "Chape - dekvloer", "Revêtement de sol - vloerafwerking" | material: "Chape"; "Parquet intérieur" | property sets: Pset_CoveringCommon, Cpset_Covering, Qto_CoveringBaseQuantities
          1 x IFCCOVERING | INSULATION | names: "Isolant - isolatie" | material: "Isolant rigide de sol" | property sets: Pset_CoveringCommon, Cpset_Covering, Qto_CoveringBaseQuantities

Property sets
  Pset_CoveringCommon | properties | on 8 objects (8 IFCCOVERING)
    Finish = "x" (IFCTEXT)
    FireRating = "x" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "x" (IFCIDENTIFIER)
    Status = "x" (IFCTEXT)
  Cpset_Covering | properties | on 8 objects (8 IFCCOVERING)
    PRReactionToFire = "x" (IFCLABEL)
    PRSoundReductionIndex = "x" (IFCLABEL)
    PRThermalConductivity = 0. (IFCTHERMALCONDUCTIVITYMEASURE)
    PRThermalResistance = 0. (IFCTHERMALRESISTANCEMEASURE)
    Phasing = "x" (IFCLABEL)
  Qto_CoveringBaseQuantities | quantities | on 8 objects (8 IFCCOVERING)
    GrossArea = 0. [CENTI SQUARE_METRE]
    NetArea = 0. [CENTI SQUARE_METRE]
    Width = 0. [CENTI METRE]
  Cpset_Ceiling | properties | on 2 objects (2 IFCCOVERING)
    ClimateCeiling = TRUE (IFCBOOLEAN)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "x" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "x" (IFCIDENTIFIER)
    Status = "x" (IFCTEXT)
  Cpset_Wall | properties | on 1 object (1 IFCWALL)
    ExternalSurfaceTreatment = "x" (IFCLABEL)
    PRReactionToFire = "x" (IFCLABEL)
    PRSoundReductionIndex = "x" (IFCLABEL)
    PRThermalConductivity = 0. (IFCTHERMALCONDUCTIVITYMEASURE)
    PRThermalResistance = 0. (IFCTHERMALRESISTANCEMEASURE)
    Phasing = "x" (IFCLABEL)
    SurfaceCharacteristics = "x" (IFCLABEL)
  Cpset_PrecastConcreteElement | properties | on 4 objects (3 IFCSLAB, 1 IFCWALL)
    CornerChamfer = 0. (IFCLENGTHMEASURE) [CENTI METRE]
  Cpset_ConcreteElementGeneral | properties | on 4 objects (3 IFCSLAB, 1 IFCWALL)
    ConstructionMethod = "x" (IFCLABEL)
    ReinforcementVolumeRatio = 0. (IFCMASSDENSITYMEASURE)
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossVolume = 0. [CENTI CUBIC_METRE]
    Height = 0. [CENTI METRE]
    Length = 0. [CENTI METRE]
    NetSideArea = 0. [CENTI SQUARE_METRE]
    NetVolume = 0. [CENTI CUBIC_METRE]
    Width = 0. [CENTI METRE]
  Pset_SlabCommon | properties | on 3 objects (3 IFCSLAB)
    FireRating = "x" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "x" (IFCIDENTIFIER)
    Status = "x" (IFCTEXT)
  Cpset_Slab | properties | on 3 objects (3 IFCSLAB)
    ExternalSurfaceTreatment = "x" (IFCLABEL)
    PRReactionToFire = "x" (IFCLABEL)
    PRSoundReductionIndex = "x" (IFCLABEL)
    PRThermalConductivity = 0. (IFCTHERMALCONDUCTIVITYMEASURE)
    PRThermalResistance = 0. (IFCTHERMALRESISTANCEMEASURE)
    Phasing = "x" (IFCLABEL)
    SurfaceCharacteristics = "x" (IFCLABEL)
  Qto_SlabBaseQuantities | quantities | on 3 objects (3 IFCSLAB)
    Depth = 0. [CENTI METRE]
    GrossArea = 0. [CENTI SQUARE_METRE]
    GrossVolume = 0. [CENTI CUBIC_METRE]
    Length = 0. [CENTI METRE]
    NetArea = 0. [CENTI SQUARE_METRE]
    NetVolume = 0. [CENTI CUBIC_METRE]
    Perimeter = 0. [CENTI METRE]
    Width = 0. [CENTI METRE]
  Pset_PrecastSlab | properties | on 3 objects (3 IFCSLAB)
    TypeDesignator = "x" (IFCLABEL)